Instructions

1. Export current configs considering all the sites including VSAT.

2. Analyse sites for VSAT and create new working set by excluding VSAT.

3. Export all the sites with new Working set.

4. Remove 1st, 3rd and 4th rows and Sort each MO on the exported file

5. Copy each MO and paste on separate files.

For example:

sheet1.csv for IKE

sheet2.csv for Week plan with Ips

sheet1\_TWAMP.csv

sheet1\_IPSECP.csv

sheet1\_SECPOL.csv

sheet1\_PROTGRP.csv

6. Check the 1st row’s labels specially for PROTGRP. ikePDN.1 and role.1 change them to ikePDN and role and check for IPRT, change labels destIpAddr.1, destinationIpPrefixLength.1, gateway.1, preSrcIpv4Addr.1, preSrcIpv4AddrDN.1, preference.1, routeIpMtu.1, triggerDN.1 to destIpAddr, destinationIpPrefixLength, gateway, preSrcIpv4Addr, preSrcIpv4AddrDN, preference, routeIpMtu, triggerDN